|  |  |
| --- | --- |
| 1軸のヒンジを採用し2つの筐体が180度まで開く構造にした場合、次のような問題が考えられる。 | If a structure is adopted in which a single-axis hinge is employed and two casings are opened to 180 degrees, problems such as the following are conceivable. |